**PC Log**

|  |  |
| --- | --- |
| **PC ID (on side of tower)** | **P1103047185 Stone Group – Core i5 2400 Sandybridge (Machine 01)** |
| **Hard Drive Capacity** | **500 GB Seagate “3.5 – SATA 3** |
| **RAM** | **8GB DDR3** |
| **Operating System** | **Kali Linux (based on Debian 8) / Windows 7 Professional** |
| **Other installed applications** | **Nmap, Wireshark, htop, SAMBA, Counter Strike: Source** |
|  |
|  |
|  |
|  |
| **Display type** | **22” iiyama Prolite – E2273HDS 1920x1080 TN LED** |
| **Components to add to existing configuration** | **Cisco Systems Catalyst 2950 Series 10/100 Base TX 1U Rackmount Switch** |
|  |
|  |

**Network Configuration (including where this asset is in this configuration)**

|  |
| --- |
| https://cdn2.iconfinder.com/data/icons/multimeda/100/desktop-512.png  https://cdn2.iconfinder.com/data/icons/multimeda/100/desktop-512.png  Ethernet Switch  Machine 02  Machine 01  http://cliparts.co/cliparts/qcB/Ayy/qcBAyyLxi.png |

**Issues (detail any issues with the hardware and/or software in this configuration)**

**The system BIOS was locked, meaning the machine couldn’t be booted. To resolve this, we moved a jumped on the motherboard to wipe the password in able to boot from a USB drive to install an operating system.**

**How issues were rectified and if not why**

**Software/Hardware needed to complete (if required)**